**Epyx FastLoad Cartridge for the C64 Rev. 2**

**Testing**

# Tests

The tests were carried out with the prototype Rev. 0 and Rev. 2. The software was stored on an AT27C256R (Atmel) and an ST M27C512 EPROM.

The Epxy FastLoad cartridge was tested with:

* ASSY 250469
* ASSY 250425
* ASSY 250407
* Ultimate 64 Elite (Firmware v1.26)

The Ultimate 64 Elite did not boot. This is a known issue. This was not tested with Rev. 2 again.

All original C64, that were tested, booted without a problem. The FDD 1541 could be accessed.

Rev. 2 was tested on ASSY250469 (the circuitry of the cartridge did not change).

* Several times switched on
* Several times reset button

The software always loaded, the menu could be loaded with the £ key. Some menu functions were tested. The directory, some 1541 commands worked and programs could be loaded.

# Conclusion

Rev. 2 is fully functional.